**MYUNG JIN SHIPPING CO., LTD.**

RM 301, 988-5, GOHYUN DONG, GEOJE, GYEONG NAM, KOREA

FLAT BARGE ‘ POS 25000’



|  |  |  |
| --- | --- | --- |
| GENERAL |  | |
| Vessel’s name | POS 25000 | |
| Builder | ForceTEC Corporation | |
| Year Built | APRIL 2009 | |
| Type | Flat Barge | |
| Classification Society | K.R(Class No. 0966705) | |
| Flag | KOREA | |
| IMO NO /Official NO / Call Sign | - / MSB-097157 / - | |
| Navigation Area | Great Coastal | |
|  |  | |
| DIMENSIONS |  | |
| LOA | 95.04 M | |
| Breadth (MLD) | 36.00 M | |
| Depth (MLD) | 6.50 M | |
| GRT / NRT | 6,190T / 1,857T | |
| Dead Weight | 12,500T | |
|  |  | |
| Tank Capacity |  | |
| IFO | - | |
| MGO | 12.0 k/l | |
| L.O |  | |
| Ballast Capacity | 2,000㎥/hr x 3EA = 6,000㎥/hr | |
| Fresh Water |  | |
|  |  | |
| PERFORMANCE | |  |
| E/R MACHINERY | |  |
| Main Generator Engine Power | | 504KW \* 1 Set |
| Aux’ Generator Engine Power | | 24KW \* 1Set |
| G.S & Fire Pump Capacity | | 90㎥/hr \* 1Set |
| BILGE & G.S Pump Capacity | | 90㎥/hr \* 1Set |
| Ventilation Fan | | 2 set |
| F.W PUMP | | 1 SET (HANIL) |
| Oily Water Separator | | 1Set (1㎥/hr \* 15ppm) |
|  | |  |
| Deck Machinery | |  |
| Anchor & Chan | | 3,540Kg \* 54￠\*9Shot \* 2Set |
| Windless | | 9m / min \* 13.0Ton 2Set |
| Windless Hyd. Pump \* Motor | | 440V \* 60Hz \* 37.0 Kw |
| MOORING WINCH | | 2 Set(10M/min \* 6.0 TON) |
|  | |  |
| Communication | |  |
| HAND V.H.F | | ICOM \* 2Set |
|  | |  |
|  | |  |
|  | |  |
|  | |  |
|  | |  |
|  | |  |

Particulars are given entirely without warranty as to correctness and interested parties must satisfy themselves by inspection of the vessel.